{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":11,"n_cols":8,"rows_kept":11,"merged":[[0,0,0,7],[2,0,7,0],[2,1,3,1],[2,7,7,7],[5,1,7,1],[9,0,9,2],[9,3,9,7],[10,0,10,7]]}
["三明生态新城智慧停车场综合体一期建设项目平行检验及幕墙工程检测报价"]
["序号","项目","内容及规格","预估\n工程量","单位","单价","小计（元）","备注"]
["平行检验","电线电缆","单芯电线（导电性能、绝缘性能、绝缘厚度、机械性能和阻燃耐火性能)",2,"组",null,null,"建设工程材料实行平行检验时，平行检验频次不少于单位工程同类材料进场检验频次的30%且不少于1次，且尽可能涵盖所有规格"]
[null,null,"多芯电缆(导电性能、绝缘性能、绝缘厚度、机械性能和阻燃耐火性能）",2,"组"]
[null,"漏电保护开关","漏电保护开关（动作时间、动作电流）",1,"个"]
[null,"有防火性能要求的保温隔热材料","岩棉板（燃烧性能A1级）",1,"组"]
[null,null,"玻璃棉板（燃烧性能B1级）",1,"组"]
[null,null,"挤塑板（燃烧性能B1级）",1,"组"]
["玻璃幕墙","幕墙四性","气密、水密、抗风压、平面内变形",1,"组"]
["总计（元）",null,null,{"$f":"SUM(G3:G9)","v":0}]
["说明：当实际检测项目超出表中所列项目范围时，可另行协商增补，按实际委托工程量结算。"]