{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":9,"n_cols":8,"rows_kept":9,"merged":[[0,0,0,7],[2,0,5,0],[2,1,3,1],[2,7,5,7],[7,0,7,2],[7,3,7,7],[8,0,8,7],[17,7,18,7]]}
["三明中关村智慧产业园标准厂房一期工程B1、A5号楼主材及性能检测技术服务费报价单"]
["序号","项目","内容及规格","预估\n工程量","单位","单价","小计（元）","备注"]
["平行检验","电线电缆","单芯电线（导电性能、绝缘性能、绝缘厚度、机械性能和阻燃耐火性能)",2,"组",null,null,"建设工程材料实行平行检验时，平行检验频次不少于单位工程同类材料进场检验频次的30%且不少于1次，且尽可能涵盖所有规格"]
[null,null,"多芯电缆(导电性能、绝缘性能、绝缘厚度、机械性能和阻燃耐火性能）",2,"组"]
[null,"漏电保护开关","漏电保护开关（动作时间、动作电流）",1,"个"]
[null,"有防火性能要求的保温隔热材料","挤塑板（燃烧性能B1级）",1,"组"]
["玻璃幕墙","幕墙四性","气密、水密、抗风压、平面内变形",1,"组"]
["总计（元）",null,null,{"$f":"SUM(G3:G7)","v":0}]
["说明：当实际检测项目超出表中所列项目范围时，可另行协商增补，按实际委托工程量结算。"]